|  |  |  |
| --- | --- | --- |
|  | **EC**  **Declaration of Conformity** | Fermax Belgium  Nieuwstraat 10  1570 Galmaarden  Tel : +32(0)54/31 92 50  Fax : +32(0)54/58 90 51 |
| Galmaarden, 1-08-2018  **Manufacturer Identification:**  Legal Name : nv Fermax Belgium sa  Address : Nieuwstraat 10  BE-1570 Galmaarden  Belgium  www.dobiss.com  Representative : Mr David Vaeremans  Function : General manager  **Product Identification:**  Product : Universal input module (0-10V/contact/pulse)  Brand : Dobiss  Model / Type : DO5480  **Declaration:**  Provided that it is installed, maintained and used in the application for which it is made, with respect of the professional practices, relevant installation codes and manufacturer’s instructions:  *We hereby declare that the above referenced product complies with the essential requirements of the following Council Directives:*  ***EMC Directive:*** *2014/30/EU*  ***Low Voltage Directive:*** *2014/35/EU*  ***RoHS Directive:*** *2011/65/EU*  ***WEEE Directive****: 2012/19/EU*  The procedures of Annex II have been applied to mark the product with the CE-label.  **European harmonised standards applied:**  EMC : EN 50491-5-1:2010 & EN 50491-5-2:2010  Product safety : EN 60950-1:2006 + A11:2009 + A1:2010 + A12:2011 + A2:2013  **Signature of manufacturer representative:**  Name:  Date: DoC identification number: EC 5480-1 | | |